DAPPING APPROVED COLORS

Graphite        #080808   Primary dark background
Off-white       #F5F5F5   Primary light and white mark
Emerald         #10B981   Verification, access, connection, completion
Bright emerald  #34D399   Small emphasis on dark backgrounds
Mineral gray    #737373   Supporting neutral

Emerald should normally occupy less than 8 percent of a composition.
